|  |  |
| --- | --- |
| VCC (IR SENSOR) | 3.3V |
| GND (IR SENSOR) | GND |
| OUT (IR SENSOR) | PD3 |
| POSTIVE(LED) | PD4 |
| NEGATIVE(LED VIA RESISTOR OF 330 OHM) | GND |

**PIN CONNECTION DETAILS**